**STILMAT EMPIRE – Carpet - open**

Text for invitation to tender

|  |  |
| --- | --- |
| Description: | Flexible and roll-up, aluminum entrance mat for laying on the floor. Custom produced mats to fit width and walking depth specifications perfectly. Suitable for wheeled traffic. Any geometric shape is available on demand. |
| Model | EMPIRE (Carpet) |
| Tread surface (inlay): | High quality dust control carpet, durable and luxurious character. Made from 100% Polyamide |
| Ideal for | Fine dirt and moisture |
| Colors: | Black, Grey, Brown… |
| Version | Open system |
| Code | TOC |
| Approx. height (mm) | 20 mm |
| Entrance position | Indoors |
| Zones: I – II - III | Zone: III |
| Load | From Normal to Heavy |
| Footfall | Daily footfall up to 2000 |
| Roll-over and drive-over capability: | Wheelchairs, Prams, Hand and Light shopping trolleys |
| Support chassis | Made from rigid anodized aluminum with rubber sound insulation underlay |
| Aluminum coating: | Fully anodized, to increase resistance to corrosion and wear. More aesthetically pleasing finish and harder surface than pure aluminum. |
| Aluminum material thickness (mm) | 1.2 |
| Connection | Strong and flexible PVC connection strip, the entire width |
| Standard profile clearance approx. (mm) | 5 mm |
| Slip resistance | R 11 slip resistance as per DIN 51130 |
| Logo options | Logo engraving |
| Contact | STILMAT |